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BASICS 
	Flag
	Bahamas

	LLoyds no.
	9206059 

	Class
	NK 1A1 Reefer

	Int GRT/NRT
	10,804 / 5,320

	Pan GRT/NRT
	- / 9,313

	Suez GRT/NRT
	11,703 / 9,710

	Built
	Japan, 1999

	Length over all m
	150.0 

	Breadth moulded m
	23.0 

	Depth W.D. m
	13.3 

	Sdwt mton
	9709

	Draught sdwt m
	9.02 

	Bale cbft
	506,228

	Area m2
	5,944.3

	Bow thruster
	N/A

	Hatch covers
	4

	Holds/Compartmens
	4/15

	Fcsle deck
	YES

	Trunk deck
	NO

	USDA
	Sensors fitted

	PPECB
	Sensors fitted

	Reefer plugs
	100

	Grating load
	6 MT Axleload

	
	Pneumatic tires

	Grating
	

	Temp min/max °C
	-25 / +15

	Air circs/hour
	90

	Air renew/hour
	2

	
	





 BALE cbft
	DECK & HATCH
	1
	2
	3
	4

	FC
	
	
	
	

	A
	42,197
	42,699
	42,515
	44,617

	B
	25,861
	35,071
	38,931
	38,323

	C
	15,630
	30,025
	37,271
	31,416

	D
	
	22,351
	34,043
	25,278

	Total
	83,688
	130,146
	152,760
	139,634


 Grand total	506,228
 DECK AREA m2	
	DECK & HATCH
	1
	2
	3
	4

	FC
	
	
	
	

	A
	462.9
	472.1
	470.3
	496.7

	B
	285.6
	423.6
	467.0
	461.0

	C
	183.7
	373.5
	465.6
	391.2

	D
	
	273.2
	409.3
	308.6

	Total
	932.2
	1542.4
	1812.2
	1657.5


 Grand total	6,226

 Free deckheight minimum 2.20 m

 HATCHES (Weather deck) m
	Hatch
	Length
	Width
	Insulated units

	
	
	
	

	1
	12.6
	7.8
	ABC

	2
	12.6
	7.8
	AB/CD

	3
	12.6
	7.8
	AB/CD

	4
	12.6
	7.8
	AB/CD


 Insulated units are separate cooling sections.



Southampton Reefer

CARGO GEAR
	No of
	Type
	SWL mton
	UP mton

	2
	Hydraulic
	40
	-

	2
	Hydraulic
	8
	-


Max single lift cap:	2 x 40 MT / 2 x 8 MT
Max twin lift cap :	N/A

MAXIMUM CONTAINER CAPACITY
	
	8’6”
	9’6”
	Stackweight (20’/40’)

	
	20 ft
	40ft
	40 ft
	No. 1
	Nos. 2-4


	Hatch covers
	80
	40
	40
	20/30
	40/60

	Weather Deck
	142
	68
	68
	20/30
	60/90

		Holds
	84
	42
	42
	40/60
	80/120*

		Totals
	306
	150
	150
	
	



100 reefer sockets on deck (20 ft and/or 40 ft)
*On tank top.  On ‘A’ deck covers 20/30 tonnes.
** Maximum reefer container capacity is 90 units at 25 tonnes gross.  Maximum container load for a particular voyage is subject  to stability, stackweight limitations, visibility from bridge and Master’s approval.
Please contact Cool Carriers for information about speed and consumption 
All details believed to be correct but not guaranteed
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